PROCEDURES  FOR BRINGING SERVERS  
                                  UP AND  DOWN

                         DOWNING THE SERVER
                     
STEP 1.        SEND THE FOLLOWING MESSAGE TO ALL USERS AT 
THE SERVER PROMPT  (HIT THE ALT ESC KEYS                                           TOGETHER) TO GET TO THE PROMPT CS-CAMDENxx:   KEY IN;                                       BROADCAST  SYSTEM  GOING  DOWN FOR                                                    MAINTENANCE IN 5 MINS .

STEP 2.        GO TO THE NOVA - STOR  BACKUP SCREEN BY HITTING                         THE (ALT ESC KEYS  AGAIN) TO GET TO THIS  SCREEN.                          HIT THE ESC KEY AND IT WILL ASK YOU IF YOU WANT                        TO EXIT NOVA NET HIT THE RETURN KEY THAT                                       HIGHLIGHTS YES.   (THIS BRINGS THE AGENT FOR                                  NOVA-STOR DOWN)

STEP 3.       GO BACK TO THE SERVER PROMPT BY HITTING THE
(ALT ESC) KEYS TOGETHER AGAIN.  KEY IN      DOWN                                 IT WILL ASK IF YOU WANT TO DOWN THE SERVER                                  THEN KEY IN Y AND HIT RETURN.  (IGNORE ANY   OPEN FILE MESSAGES.)

STEP 4.        THE SERVER SHOULD COME BACK AND SAY IT IS                                      DOWN AND LEAVE YOU AT A  C:\subdir  PROMPT.   IF IT DOESN’T AFTER ABOUT 10 MINS.  TURN THE GREEN LIGHT BUTTON OFF ON THE APPROPRIATE SERVER, (PUSH IN AND LET GO AND                                WAIT ABOUT 30 SECS.  BEFORE YOU TURN IT ON                                     AGAIN, BY PUSHING THE BUTTON IN.  

	            BRINGING THE SERVER UP

STEP 1.        TURN THE SERVER ON BY PUSHING IN THE ON OFF                                  BUTTON THE GREEN LIGHT SHOULD COME ON.   THE  SYSTOM WILL TAKE A FEW MINUTES TO RUN ITS DRIVE CHECKS.               

STEP 2.        A SCREEN WILL COME UP WITH A “DOS” PROMPT WHERE IT WILL ASK YOU TO TYPE IN AN S KEY AND IT WILL RUN  A .BAT FILE THAT WILL START THE SERVER PROGRAM.

STEP 3.        AS THE SERVER IS COMING UP IT MIGHT ASK FOR A                                  PASSWORD FOR ED MCHUGH JUST HIT ESC THIS WILL                          BY PASS THIS QUESTION. 

STEP 4.        THE FINAL STEP IS BRINGING UP NOVA STOR.   AFTER                           THE SERVER IS UP GO TO A SCREEN THAT HAS A SERVER PROMPT   CS-CAMDENxx.  HIT THE ALT ESC KEYS TOGETHER TO GET TO IT.   KEY IN NNAGENT, A BLUE SCREEN APPEARS AND IT WILL SAY NOVA NET AGENT FOR NETWARE.   THIS MEANS THE BACKUP AGENT IS  RUNNING.   

STEP 5.        SCROLL THROUGH MENU HIT THE ALT ESC KEYS TOGETHER .  CHECK THAT  PRINTER AGENTS ARE UP INCLUDING:
   THE  BROKER  SCREEN -        LOAD BROKER “CAMPRINTx.RUCS”  WHERE THE   “  AND  ” ARE NEEDED AND THE  x  IS THE SERVER NUMBER AS IN “CAMPRINT1.RUCS” OR “CAMPRINT2.RUCS”
   THE NDPS MANAGER -        LOAD NDPSM “CAMMANx”   
WHERE THE   “  AND  ” ARE NEEDED AND THE  x  IS THE SERVER
NUMBER AS IN  “CAMMAN4”
   THE HEWLETT-PACKARD NDPS GATEWAY SCREEN – WHICH GETS LOADED BY THE  ABOVE COMMAND
WITH THESE LOADED THE SYSTEM IS READY FOR USAGE.

STEP 6.        DONE.                    

OIT JULY 5, 2001